.TH "rtcNewBVH" "3" "" "" "Embree Ray Tracing Kernels 3"
.SS NAME
.IP
.nf
\f[C]
rtcNewBVH\ \-\ creates\ a\ new\ BVH\ object
\f[]
.fi
.SS SYNOPSIS
.IP
.nf
\f[C]
#include\ <embree3/rtcore.h>

RTCBVH\ rtcNewBVH(RTCDevice\ device);
\f[]
.fi
.SS DESCRIPTION
.PP
This function creates a new BVH object and returns a handle to this BVH.
The BVH object is reference counted with an initial reference count of
1.
The handle can be released using the \f[C]rtcReleaseBVH\f[] API call.
.PP
The BVH object can be used to build a BVH in a user\-specified format
over user\-specified primitives.
See the documentation of the \f[C]rtcBuildBVH\f[] call for more details.
.SS EXIT STATUS
.PP
On failure an error code is set that can be queried using
\f[C]rtcGetDeviceError\f[].
.SS SEE ALSO
.PP
[rtcRetainBVH], [rtcReleaseBVH], [rtcBuildBVH]
